<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="131.445" y1="10" x2="131.445" y2="95.791" width="0" layer="20"/>
<wire x1="131.445" y1="95.791" x2="121.445" y2="105.791" width="0" layer="20" curve="90"/>
<wire x1="121.445" y1="105.791" x2="10" y2="105.791" width="0" layer="20"/>
<wire x1="10" y1="105.791" x2="0" y2="95.791" width="0" layer="20" curve="90"/>
<wire x1="27.4" y1="0" x2="10" y2="0" width="0" layer="20"/>
<wire x1="10" y1="0" x2="0" y2="10" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="10" x2="0" y2="95.791" width="0" layer="20"/>
<wire x1="113.14" y1="0" x2="121.445" y2="0" width="0" layer="20"/>
<wire x1="121.445" y1="0" x2="131.445" y2="10" width="0" layer="20" curve="90"/>
<text>DIO</text>
<text>CLK</text>
<text>OpenEnergyMonitor</text>
<text>Development Board</text>
<text>emonSTM32</text>
<text>v0.7</text>
<text>Designed in </text>
<text>North Wales </text>
<text>Made in UK</text>
<hole x="126.49" y="100.85" drill="3.5"/>
<hole x="4.95" y="100.85" drill="3.5"/>
<hole x="4.95" y="4.95" drill="3.5"/>
<hole x="126.49" y="4.95" drill="3.5"/>
<text>VT3</text>
<text>VT2</text>
<text>VT1</text>
<text>131.445 x
105.791 y</text>
<wire x1="27.4" y1="19.066" x2="80.407" y2="19.066" width="0" layer="20"/>
<wire x1="80.407" y1="19.066" x2="80.407" y2="0" width="0" layer="20"/>
<text>Open Hardware</text>
<wire x1="27.4" y1="19.066" x2="27.4" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>MCP1501</text>
<text>GND</text>
<wire x1="113.14" y1="0" x2="113.14" y2="2" width="0" layer="20"/>
<wire x1="105.14" y1="0" x2="105.14" y2="2" width="0" layer="20"/>
<wire x1="105.14" y1="2" x2="113.14" y2="2" width="0" layer="20"/>
<wire x1="80.407" y1="0" x2="105.14" y2="0" width="0" layer="20"/>
<text>UART_ESP</text>
<text>CH291-1220LF</text>
<text>TB1</text>
<text>TB2</text>
<text>TB3</text>
<text>TB5</text>
<text>TB4</text>
<text>RJ1</text>
<text>RJ2</text>
<text>UART_STM</text>
<text>OpenEnergyMonitor</text>
<text>Development Board</text>
<text>emonSTM32</text>
<text>v0.7</text>
<text>3V3</text>
<text>BIAS</text>
<text>RST</text>
<text>Tx</text>
<text>Rx</text>
<text>5V</text>
<text>3V3</text>
</plain>
<libraries>
<library name="SteelCaveRobotics-Power">
<description>&lt;h3&gt;Steel Cave Robotics Eagle Libraries - Power&lt;/h3&gt;
&lt;a href="https://github.com/steelcaverobotics/SteelCaveRobotics-Eagle-Libraries"&gt;https://github.com/steelcaverobotics/SteelCaveRobotics-Eagle-Libraries&lt;/a&gt;</description>
<packages>
<package name="SOT-223">
<description>SOT-223-3</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="1X02">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="IotaWatt_parts">
<packages>
<package name="STEREO_SMT">
<description>stereo 3.5mm SMD</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="DCJACK_2MM_SMT">
<description>2.0/2.1mm DC Jack - SMT
&lt;p&gt;4UConnector: 03267&lt;/p&gt;
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_6X200_NOTEXT">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
</packages>
</library>
<library name="stm32f303">
<packages>
<package name="TQFP100">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="CRYSTAL_8X3.8">
<description>&lt;p&gt;8.0x3.8x2.5mm SMT Crystal&lt;/p&gt;
&lt;p&gt;Source: http://www.abracon.com/Resonators/abs25.pdf&lt;/p&gt;</description>
</package>
<package name="SOD-523">
<description>SOD-523 (0.8x1.2mm)

&lt;p&gt;Source: http://www.rohm.com/products/databook/di/pdf/rb751s-40.pdf&lt;/p&gt;</description>
</package>
<package name="SOT23-R">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Reflow soldering</description>
</package>
</packages>
</library>
<library name="e14_Rpi3_RevA+mirror-pcb copy">
<packages>
<package name="RPI3MIRROR2">
</package>
</packages>
</library>
<library name="rfm12b _ rfm69cw">
<packages>
<package name="RFM12">
</package>
</packages>
</library>
<library name="MCP1501T-33E">
<packages>
<package name="SOT95P280X145-6N">
</package>
</packages>
</library>
<library name="Transistor">
<description>PCBLayout.com - General purpose Transistors</description>
<packages>
<package name="SOT23">
<description>Small Outline Transistor (SOT23), 0.95 mm pitch; 3 pin, 2.92 mm L X 1.325 mm W X 1.20 mm H body&lt;p&gt;&lt;i&gt;PCB Libraries Packages&lt;/i&gt;</description>
</package>
</packages>
</library>
<library name="BOOST MODULE CN6009">
<packages>
<package name="BOOST">
</package>
</packages>
</library>
<library name="smd-special">
<description>&lt;b&gt;Special SMD Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMS-001">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ESP32-WROOM-32D">
<packages>
<package name="MODULE_ESP32-WROOM-32D">
</package>
</packages>
</library>
<library name="pinhead+">
<packages>
<package name="2X13_SMT">
</package>
</packages>
</library>
<library name="95501-6889 rj45 smt">
<description>&lt;Molex Cat3 8-Way Female RJ45 Connector Right Angle Surface Mount Unshielded&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="955016889">
<description>&lt;b&gt;95501-6889-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="KSS221GLFS">
<description>&lt;IP40 Side Tactile Switch, SPST-NO 50 mA&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="KSS">
<description>&lt;b&gt;KSS&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="CSP-USC16-TR">
<packages>
<package name="USB-C">
</package>
</packages>
</library>
<library name="3.5mm terminal block rs pro">
<packages>
<package name="3.5MM_X3">
</package>
</packages>
</library>
<library name="CH291-1220LF">
<packages>
<package name="CH291-1220LF">
<description>&lt;b&gt;Battery Holder, SMT, 12mm&lt;/b&gt;&lt;p&gt;
multicomp PART NO. CH291-1220LF&lt;br&gt;
Source: &lt;a href="http://www.farnell.com/datasheets/1505860.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb-db">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA04-1-OLED">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA06-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_1-NC_TRACE_NO-SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MCP1825" library="SteelCaveRobotics-Power" package="SOT-223" value="MCP1825SOT-223-3">
<attribute name="NAME"/>
</element>
<element name="C3" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C4" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C6" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C8" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C9" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="BOOT_STM" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CT9" library="IotaWatt_parts" package="STEREO_SMT" value="SJ-3523-SMT">
<attribute name="MPN" value="SJ-3523-SMT"/>
<attribute name="NAME"/>
</element>
<element name="RB1" library="rcl" package="R1206" value="22r">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="41"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="RF1" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
</element>
<element name="CF1" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="CT8" library="IotaWatt_parts" package="STEREO_SMT" value="SJ-3523-SMT">
<attribute name="MPN" value="SJ-3523-SMT"/>
<attribute name="NAME"/>
</element>
<element name="RB2" library="rcl" package="R1206" value="22r">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="41"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="RF2" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
</element>
<element name="CF2" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="CT7" library="IotaWatt_parts" package="STEREO_SMT" value="SJ-3523-SMT">
<attribute name="MPN" value="SJ-3523-SMT"/>
<attribute name="NAME"/>
</element>
<element name="RB3" library="rcl" package="R1206" value="22r">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="41"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="RF3" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
</element>
<element name="CF3" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="RV3" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
</element>
<element name="CV3" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="R51" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R41" library="resistor" package="R0603" value="120k">
<attribute name="NAME"/>
</element>
<element name="R22" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50*" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="HSE" library="crystal" package="CTS406" value="406C35E08M00000">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="LED1" library="adafruit" package="CHIP-LED0805" value="Green 1.85V">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="ohw-logo" package="OSHW_6X200_NOTEXT" value="OSHW_LOGO_6MILX0200-NT"/>
<element name="VT3" library="adafruit" package="DCJACK_2MM_SMT" value="ADC-028-2-T">
<attribute name="MPN" value="ADC-028-1-T"/>
</element>
<element name="SJ1" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="CT4" library="IotaWatt_parts" package="STEREO_SMT" value="SJ-3523-SMT">
<attribute name="MPN" value="SJ-3523-SMT"/>
<attribute name="NAME"/>
</element>
<element name="CT5" library="IotaWatt_parts" package="STEREO_SMT" value="SJ-3523-SMT">
<attribute name="MPN" value="SJ-3523-SMT"/>
<attribute name="NAME"/>
</element>
<element name="CT6" library="IotaWatt_parts" package="STEREO_SMT" value="SJ-3523-SMT">
<attribute name="MPN" value="SJ-3523-SMT"/>
<attribute name="NAME"/>
</element>
<element name="CT3" library="IotaWatt_parts" package="STEREO_SMT" value="SJ-3523-SMT">
<attribute name="MPN" value="SJ-3523-SMT"/>
<attribute name="NAME"/>
</element>
<element name="CT2" library="IotaWatt_parts" package="STEREO_SMT" value="SJ-3523-SMT">
<attribute name="MPN" value="SJ-3523-SMT"/>
<attribute name="NAME"/>
</element>
<element name="CT1" library="IotaWatt_parts" package="STEREO_SMT" value="SJ-3523-SMT">
<attribute name="MPN" value="SJ-3523-SMT"/>
<attribute name="MPN" value="SJ-3523-SMT"/>
<attribute name="NAME"/>
</element>
<element name="VT2" library="adafruit" package="DCJACK_2MM_SMT" value="ADC-028-2-T">
<attribute name="MPN" value="ADC-028-1-T"/>
</element>
<element name="VT1" library="adafruit" package="DCJACK_2MM_SMT" value="ADC-028-2-T">
<attribute name="MPN" value="ADC-028-1-T"/>
</element>
<element name="RJ45_1" library="95501-6889 rj45 smt" package="955016889" value="95501-6889">
<attribute name="ALLIED_NUMBER" value="70372913"/>
<attribute name="ALLIED_PRICE-STOCK" value="https://www.alliedelec.com/molex-incorporated-95501-6889/70372913/"/>
<attribute name="DESCRIPTION" value="Molex Cat3 8-Way Female RJ45 Connector Right Angle Surface Mount Unshielded"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="95501-6889"/>
<attribute name="MOUSER_PART_NUMBER" value="538-95501-6889"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=538-95501-6889"/>
<attribute name="NAME"/>
<attribute name="RS_PART_NUMBER" value="3862738"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/3862738"/>
</element>
<element name="STM32F303VE" library="stm32f303" package="TQFP100" value="STM32F303VE">
<attribute name="MPN" value="STM32F303VET6"/>
<attribute name="NAME"/>
</element>
<element name="R42" library="resistor" package="R0603" value="120k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="resistor" package="R0603" value="120k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RV2" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RV1" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CV2" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CV1" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RB4" library="rcl" package="R1206" value="22r">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="41"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RF4" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF4" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RB5" library="rcl" package="R1206" value="22r">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="41"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RF5" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF5" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RB6" library="rcl" package="R1206" value="22r">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="41"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RF6" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF6" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RB7" library="rcl" package="R1206" value="22r">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="41"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RF7" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF7" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RB8" library="rcl" package="R1206" value="22r">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="41"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RF8" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF8" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RB9" library="rcl" package="R1206" value="22r">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="41"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RF9" library="resistor" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF9" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LSE" library="microbuilder" package="CRYSTAL_8X3.8" value="32.768kHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RFM69HCW" library="rfm12b _ rfm69cw" package="RFM12" value="RFM12_SMDSMD"/>
<element name="R4" library="rcl" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="LED2" library="adafruit" package="CHIP-LED0805" value="Orange 1.85V">
<attribute name="NAME"/>
</element>
<element name="R5" library="rcl" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="LED3" library="adafruit" package="CHIP-LED0805" value="Red 1.85V">
<attribute name="NAME"/>
</element>
<element name="J$1" library="SparkFun-Connectors" package="SMA-EDGE" value="SMA_EDGE"/>
<element name="PCB2" library="e14_Rpi3_RevA+mirror-pcb copy" package="RPI3MIRROR2" value="TSM-120-01-T-DV">
<attribute name="MPN" value="M20-7872042"/>
</element>
<element name="VREF_3V3" library="MCP1501T-33E" package="SOT95P280X145-6N" value="MCP1501T-33E"/>
<element name="SJ2" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="C2" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ5" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ6" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ7" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ8" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="R9" library="rcl" package="R0603" value="39K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0603" value="33K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0603" value="22K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0603" value="3k3">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0603" value="82R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0603" value="220K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="SJ11" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ12" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Transistor" package="SOT23" value="MMBT3906">
<attribute name="CREATED_BY" value="PCB Layout"/>
<attribute name="DIGIKEY_PART_NUMBER" value="MMBT3906FSCT-ND"/>
<attribute name="MANUFACTURER" value="ON Semiconductor"/>
<attribute name="MPN" value="MMBT3906"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="Transistor" package="SOT23" value="MMBT3904">
<attribute name="CREATED_BY" value="PCB Layout"/>
<attribute name="DIGIKEY_PART_NUMBER" value="MMBT3904FSCT-ND"/>
<attribute name="MANUFACTURER" value="ON Semiconductor"/>
<attribute name="MPN" value="MMBT3904"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Transistor" package="SOT23" value="MMBT3904">
<attribute name="CREATED_BY" value="PCB Layout"/>
<attribute name="DIGIKEY_PART_NUMBER" value="MMBT3904FSCT-ND"/>
<attribute name="MANUFACTURER" value="ON Semiconductor"/>
<attribute name="MPN" value="MMBT3904"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="BOOST MODULE CN6009" package="BOOST" value="BOOST_MODULE"/>
<element name="RB10" library="rcl" package="0207/7" value="22r">
<attribute name="POPULARITY" value="46"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RB11" library="rcl" package="0207/7" value="22r">
<attribute name="POPULARITY" value="46"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RB12" library="rcl" package="0207/7" value="22r">
<attribute name="POPULARITY" value="46"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RB13" library="rcl" package="0207/7" value="22r">
<attribute name="POPULARITY" value="46"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RB14" library="rcl" package="0207/7" value="22r">
<attribute name="POPULARITY" value="46"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RB15" library="rcl" package="0207/7" value="22r">
<attribute name="POPULARITY" value="46"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RB16" library="rcl" package="0207/7" value="22r">
<attribute name="POPULARITY" value="46"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RB17" library="rcl" package="0207/7" value="22r">
<attribute name="POPULARITY" value="46"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="RB18" library="rcl" package="0207/7" value="22r">
<attribute name="POPULARITY" value="46"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="EXPANSION" library="pinhead+" package="2X13_SMT" value="TSM-113-01-T-DV">
<attribute name="MANUFACTURER" value="SAMTEC"/>
<attribute name="MPN" value="TSM-113-01-T-DV"/>
<attribute name="VALUE"/>
</element>
<element name="S33" library="smd-special" package="SMS-001" value="SWS001">
<attribute name="MPN" value="SDA01H1SBD"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S22" library="smd-special" package="SMS-001" value="SWS001">
<attribute name="MPN" value="SDA01H1SBD"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S11" library="smd-special" package="SMS-001" value="SWS001">
<attribute name="MPN" value="SDA01H1SBD"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="CHIP-LED0805" value="Green 1.85V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="ESP32-WROOM-32D" package="MODULE_ESP32-WROOM-32D" value="ESP32-WROOM-32D">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" IC: SoC; GPIO, I2C, I2S, IR, SD, SDIO, SPI, UART; 2.7÷3.6VDC; 20dBm "/>
<attribute name="MF" value="Espressif Systems"/>
<attribute name="MP" value="ESP32-WROOM-32D"/>
<attribute name="PACKAGE" value="Module Espressif Systems"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BOOT_ESP" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SJ9" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SJ10" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SJ13" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SJ14" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SJ15" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SJ16" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SJ17" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="D1" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D12" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="microbuilder" package="SOT23-R" value="">
<attribute name="MPN" value="NTR5103NT1G"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ18" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="SJ19" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ20" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ21" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="D22" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D23" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="KSS221GLFS" package="KSS" value="KSS221GLFS">
<attribute name="DESCRIPTION" value="IP40 Side Tactile Switch, SPST-NO 50 mA"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="C &amp; K COMPONENTS"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="KSS221GLFS"/>
<attribute name="NAME"/>
<attribute name="RS_PART_NUMBER" value="7931689P"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/7931689P"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="KSS221GLFS" package="KSS" value="KSS221GLFS">
<attribute name="DESCRIPTION" value="IP40 Side Tactile Switch, SPST-NO 50 mA"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="C &amp; K COMPONENTS"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="KSS221GLFS"/>
<attribute name="NAME"/>
<attribute name="RS_PART_NUMBER" value="7931689P"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/7931689P"/>
<attribute name="VALUE"/>
</element>
<element name="UART1" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB-C" library="CSP-USC16-TR" package="USB-C" value="CSP-USC16-TR">
<attribute name="MPN" value="CSP-USC16-TR"/>
</element>
<element name="TP4" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="POPULARITY" value="19"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="POPULARITY" value="19"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="POPULARITY" value="19"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="RJ45_2" library="95501-6889 rj45 smt" package="955016889" value="95501-6889">
<attribute name="ALLIED_NUMBER" value="70372913"/>
<attribute name="ALLIED_PRICE-STOCK" value="https://www.alliedelec.com/molex-incorporated-95501-6889/70372913/"/>
<attribute name="DESCRIPTION" value="Molex Cat3 8-Way Female RJ45 Connector Right Angle Surface Mount Unshielded"/>
<attribute name="HEIGHT" value="11.5mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="95501-6889"/>
<attribute name="MOUSER_PART_NUMBER" value="538-95501-6889"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=538-95501-6889"/>
<attribute name="NAME"/>
<attribute name="RS_PART_NUMBER" value="3862738"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/3862738"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="3.5mm terminal block rs pro" package="3.5MM_X3" value="3.5MM_TERMINAL_BLOCK">
<attribute name="MPN" value="144-4326"/>
<attribute name="RS_PART_NUMBER" value="144-4326"/>
</element>
<element name="U$3" library="3.5mm terminal block rs pro" package="3.5MM_X3" value="3.5MM_TERMINAL_BLOCK">
<attribute name="MPN" value="144-4326"/>
<attribute name="RS_PART_NUMBER" value="144-4326"/>
</element>
<element name="U$4" library="3.5mm terminal block rs pro" package="3.5MM_X3" value="3.5MM_TERMINAL_BLOCK">
<attribute name="MPN" value="144-4326"/>
<attribute name="RS_PART_NUMBER" value="144-4326"/>
</element>
<element name="U$5" library="3.5mm terminal block rs pro" package="3.5MM_X3" value="3.5MM_TERMINAL_BLOCK">
<attribute name="MPN" value="144-4326"/>
<attribute name="RS_PART_NUMBER" value="144-4326"/>
</element>
<element name="U$6" library="3.5mm terminal block rs pro" package="3.5MM_X3" value="3.5MM_TERMINAL_BLOCK">
<attribute name="MPN" value="144-4326"/>
<attribute name="RS_PART_NUMBER" value="144-4326"/>
</element>
<element name="SJ23" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ24" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ25" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ26" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ27" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="C1" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D17" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D18" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D21" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="resistor" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D26" library="microbuilder" package="SOD-523" value="ESD5Z3.3T1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ST_LINK" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="resistor" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OLED" library="con-lstb-db" package="MA04-1-OLED" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ28" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ29" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ30" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="SJ32" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="G1" library="CH291-1220LF" package="CH291-1220LF" value="CH291-1220LF">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" BATTERY HOLDER, SMT, 12MM; Accessory Type: Coin Cell Battery Holder; For Use With: 1220 Coin Cell Batteries; Battery ... "/>
<attribute name="MF" value="Multicomp"/>
<attribute name="MP" value="CH291-1220LF"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="resistor" package="R0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D40*1" library="microbuilder" package="SOD-523" value="ESD5Z5.0T1G">
<attribute name="VALUE"/>
</element>
<element name="SJ31" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="SJ33" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-lstb-db" package="MA06-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV2" library="con-lstb-db" package="MA06-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="resistor" package="R0603" value="200k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0603" value="200pF*">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="rcl" package="C0603" value="5nF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl" package="C0603" value="5nF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_TRACE_NO-SILK" value="JUMPER-SMT_3_1-NC_TRACE_NO-SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="MCP1825" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="CF1" pad="1"/>
<contactref element="CF2" pad="1"/>
<contactref element="CF3" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="C50*" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="STM32F303VE" pad="20"/>
<contactref element="STM32F303VE" pad="49"/>
<contactref element="STM32F303VE" pad="74"/>
<contactref element="STM32F303VE" pad="99"/>
<contactref element="CF4" pad="1"/>
<contactref element="CF5" pad="1"/>
<contactref element="CF6" pad="1"/>
<contactref element="CF7" pad="1"/>
<contactref element="CF8" pad="1"/>
<contactref element="CF9" pad="1"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="J$1" pad="GND@3"/>
<contactref element="J$1" pad="GND@2"/>
<contactref element="J$1" pad="GND@1"/>
<contactref element="J$1" pad="GND@0"/>
<contactref element="MCP1825" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="PCB2" pad="P$46"/>
<contactref element="PCB2" pad="P$54"/>
<contactref element="PCB2" pad="P$60"/>
<contactref element="PCB2" pad="P$70"/>
<contactref element="PCB2" pad="P$74"/>
<contactref element="PCB2" pad="P$79"/>
<contactref element="PCB2" pad="P$65"/>
<contactref element="PCB2" pad="P$49"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="RJ45_1" pad="1"/>
<contactref element="RJ45_1" pad="3"/>
<contactref element="RJ45_1" pad="5"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="RFM69HCW" pad="7"/>
<contactref element="RFM69HCW" pad="10"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="VREF_3V3" pad="2"/>
<contactref element="VREF_3V3" pad="5"/>
<contactref element="VREF_3V3" pad="3"/>
<contactref element="C13" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="EXPANSION" pad="1"/>
<contactref element="EXPANSION" pad="14"/>
<contactref element="LED4" pad="C"/>
<contactref element="U1" pad="39"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="38"/>
<contactref element="U1" pad="15"/>
<contactref element="BOOT_ESP" pad="1"/>
<contactref element="D4" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="D1" pad="A"/>
<contactref element="D5" pad="A"/>
<contactref element="D6" pad="A"/>
<contactref element="D7" pad="A"/>
<contactref element="D9" pad="A"/>
<contactref element="D8" pad="A"/>
<contactref element="D11" pad="A"/>
<contactref element="D12" pad="A"/>
<contactref element="D13" pad="A"/>
<contactref element="Q4" pad="1"/>
<contactref element="D10" pad="A"/>
<contactref element="D22" pad="A"/>
<contactref element="D23" pad="A"/>
<contactref element="C24" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="USB-C" pad="A1/B12"/>
<contactref element="USB-C" pad="B1/A12"/>
<contactref element="USB-C" pad="GND2"/>
<contactref element="USB-C" pad="GND1"/>
<contactref element="USB-C" pad="GND3"/>
<contactref element="USB-C" pad="GND4"/>
<contactref element="U1" pad="31"/>
<contactref element="C45" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="RJ45_2" pad="1"/>
<contactref element="RJ45_2" pad="3"/>
<contactref element="RJ45_2" pad="5"/>
<contactref element="CV3" pad="2"/>
<contactref element="CV2" pad="2"/>
<contactref element="CV1" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="D21" pad="A"/>
<contactref element="D18" pad="A"/>
<contactref element="D17" pad="A"/>
<contactref element="D26" pad="A"/>
<contactref element="C22" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="G1" pad="-"/>
<contactref element="OLED" pad="4"/>
<contactref element="D40*1" pad="A"/>
<contactref element="C15" pad="1"/>
<contactref element="SV2" pad="1"/>
<contactref element="SV1" pad="1"/>
<contactref element="EXPANSION" pad="25"/>
<contactref element="EXPANSION" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U$3" pad="P$3"/>
<contactref element="U$4" pad="P$3"/>
<contactref element="U$5" pad="P$3"/>
<contactref element="U$6" pad="P$3"/>
<contactref element="C23" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C31" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="PCB2" pad="P$44"/>
<contactref element="PCB2" pad="P$42"/>
<contactref element="RJ45_1" pad="7"/>
<contactref element="U$2" pad="IN+"/>
<contactref element="C18" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C42" pad="1"/>
<contactref element="USB-C" pad="A4/B9"/>
<contactref element="USB-C" pad="B4/A9"/>
<contactref element="TP4" pad="TP"/>
<contactref element="C47" pad="1"/>
<contactref element="RJ45_2" pad="7"/>
<contactref element="C7" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="VREF_3V3" pad="6"/>
<contactref element="VREF_3V3" pad="4"/>
<contactref element="C15" pad="2"/>
<contactref element="SV2" pad="3"/>
<contactref element="SV1" pad="3"/>
<contactref element="EXPANSION" pad="26"/>
<contactref element="D40*1" pad="K"/>
<contactref element="C3" pad="1"/>
<contactref element="MCP1825" pad="1"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="MCP1825" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="BOOT_STM" pad="2"/>
<contactref element="SJ1" pad="2"/>
<contactref element="STM32F303VE" pad="28"/>
<contactref element="STM32F303VE" pad="50"/>
<contactref element="STM32F303VE" pad="75"/>
<contactref element="STM32F303VE" pad="100"/>
<contactref element="RFM69HCW" pad="9"/>
<contactref element="SJ2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="RJ45_1" pad="2"/>
<contactref element="STM32F303VE" pad="22"/>
<contactref element="C13" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="EXPANSION" pad="4"/>
<contactref element="R10" pad="2"/>
<contactref element="Q4" pad="3"/>
<contactref element="EXPANSION" pad="24"/>
<contactref element="D23" pad="K"/>
<contactref element="D22" pad="K"/>
<contactref element="C40" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="RJ45_2" pad="2"/>
<contactref element="SJ23" pad="2"/>
<contactref element="C26" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="OLED" pad="3"/>
<contactref element="R13" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="BOOT0">
<contactref element="BOOT_STM" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="STM32F303VE" pad="94"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="STM32F303VE" pad="6"/>
<contactref element="G1" pad="+"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="SWDIO">
<contactref element="STM32F303VE" pad="72"/>
<contactref element="ST_LINK" pad="2"/>
</signal>
<signal name="SWCLK">
<contactref element="STM32F303VE" pad="76"/>
<contactref element="ST_LINK" pad="1"/>
</signal>
<signal name="BIAS">
<contactref element="R51" pad="2"/>
<contactref element="VT3" pad="GND"/>
<contactref element="VT3" pad="GNDBREAK"/>
<contactref element="VT2" pad="GND"/>
<contactref element="VT2" pad="GNDBREAK"/>
<contactref element="VT1" pad="GND"/>
<contactref element="VT1" pad="GNDBREAK"/>
<contactref element="R52" pad="2"/>
<contactref element="R53" pad="2"/>
<contactref element="RB4" pad="2"/>
<contactref element="CT6" pad="P$1"/>
<contactref element="RB5" pad="2"/>
<contactref element="CT5" pad="P$1"/>
<contactref element="RB6" pad="2"/>
<contactref element="CT4" pad="P$1"/>
<contactref element="CT3" pad="P$1"/>
<contactref element="RB13" pad="2"/>
<contactref element="RB14" pad="2"/>
<contactref element="RB15" pad="2"/>
<contactref element="STM32F303VE" pad="51"/>
<contactref element="CT9" pad="P$1"/>
<contactref element="RB1" pad="2"/>
<contactref element="RB10" pad="2"/>
<contactref element="CT8" pad="P$1"/>
<contactref element="RB2" pad="2"/>
<contactref element="RB11" pad="2"/>
<contactref element="CT7" pad="P$1"/>
<contactref element="RB3" pad="2"/>
<contactref element="RB12" pad="2"/>
<contactref element="S11" pad="2"/>
<contactref element="CT1" pad="P$1"/>
<contactref element="S22" pad="2"/>
<contactref element="CT2" pad="P$1"/>
<contactref element="S33" pad="2"/>
<contactref element="D1" pad="K"/>
<contactref element="CT9" pad="P$4"/>
<contactref element="CT4" pad="P$4"/>
<contactref element="CT3" pad="P$4"/>
<contactref element="CT2" pad="P$4"/>
<contactref element="CT5" pad="P$4"/>
<contactref element="CT8" pad="P$4"/>
<contactref element="CT7" pad="P$4"/>
<contactref element="CT6" pad="P$4"/>
<contactref element="CT1" pad="P$4"/>
</signal>
<signal name="N$2">
<contactref element="CT9" pad="P$2"/>
<contactref element="RB1" pad="1"/>
<contactref element="RF1" pad="1"/>
<contactref element="RB10" pad="1"/>
<contactref element="D5" pad="K"/>
</signal>
<signal name="N$8">
<contactref element="CT8" pad="P$2"/>
<contactref element="RB2" pad="1"/>
<contactref element="RF2" pad="1"/>
<contactref element="RB11" pad="1"/>
<contactref element="D6" pad="K"/>
</signal>
<signal name="N$10">
<contactref element="CT7" pad="P$2"/>
<contactref element="RB3" pad="1"/>
<contactref element="RF3" pad="1"/>
<contactref element="RB12" pad="1"/>
<contactref element="D7" pad="K"/>
</signal>
<signal name="ADC0">
<contactref element="R51" pad="1"/>
<contactref element="R41" pad="2"/>
<contactref element="RV3" pad="1"/>
</signal>
<signal name="AC3">
<contactref element="R41" pad="1"/>
<contactref element="VT3" pad="PWR2"/>
</signal>
<signal name="VSIG1">
<contactref element="STM32F303VE" pad="23"/>
<contactref element="RV1" pad="2"/>
<contactref element="D2" pad="K"/>
<contactref element="CV1" pad="1"/>
</signal>
<signal name="CT1">
<contactref element="RF1" pad="2"/>
<contactref element="CF1" pad="2"/>
<contactref element="STM32F303VE" pad="44"/>
</signal>
<signal name="CT2">
<contactref element="RF2" pad="2"/>
<contactref element="CF2" pad="2"/>
<contactref element="STM32F303VE" pad="43"/>
</signal>
<signal name="CT3">
<contactref element="CF3" pad="2"/>
<contactref element="RF3" pad="2"/>
<contactref element="STM32F303VE" pad="42"/>
</signal>
<signal name="BIAS_IN">
<contactref element="C50*" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="STM32F303VE" pad="58"/>
</signal>
<signal name="HSE_IN">
<contactref element="HSE" pad="1"/>
<contactref element="STM32F303VE" pad="12"/>
<contactref element="C30" pad="1"/>
</signal>
<signal name="HSE_OUT">
<contactref element="STM32F303VE" pad="13"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="DS18B20_RJ45">
<contactref element="RJ45_1" pad="4"/>
<contactref element="STM32F303VE" pad="66"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="R3" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="UART2_TX">
<contactref element="STM32F303VE" pad="86"/>
<contactref element="STM32F303VE" pad="25"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$1">
<contactref element="SJ1" pad="1"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="R42" pad="1"/>
<contactref element="RV2" pad="1"/>
<contactref element="R52" pad="1"/>
</signal>
<signal name="AC2">
<contactref element="R42" pad="2"/>
<contactref element="VT2" pad="PWR2"/>
</signal>
<signal name="AC1">
<contactref element="VT1" pad="PWR2"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="R43" pad="1"/>
<contactref element="RV1" pad="1"/>
<contactref element="R53" pad="1"/>
</signal>
<signal name="VSIG2">
<contactref element="RV2" pad="2"/>
<contactref element="STM32F303VE" pad="24"/>
<contactref element="D3" pad="K"/>
<contactref element="CV2" pad="1"/>
</signal>
<signal name="VSIG3">
<contactref element="RV3" pad="2"/>
<contactref element="D4" pad="K"/>
<contactref element="STM32F303VE" pad="27"/>
<contactref element="CV3" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="RB4" pad="1"/>
<contactref element="RF4" pad="1"/>
<contactref element="CT6" pad="P$2"/>
<contactref element="RB15" pad="1"/>
<contactref element="D8" pad="K"/>
</signal>
<signal name="N$39">
<contactref element="RB5" pad="1"/>
<contactref element="RF5" pad="1"/>
<contactref element="CT5" pad="P$2"/>
<contactref element="RB14" pad="1"/>
<contactref element="D9" pad="K"/>
</signal>
<signal name="N$40">
<contactref element="RB6" pad="1"/>
<contactref element="RF6" pad="1"/>
<contactref element="CT4" pad="P$2"/>
<contactref element="RB13" pad="1"/>
<contactref element="D10" pad="K"/>
</signal>
<signal name="N$42">
<contactref element="RB7" pad="1"/>
<contactref element="RF7" pad="1"/>
<contactref element="CT3" pad="P$2"/>
<contactref element="RB16" pad="1"/>
<contactref element="D11" pad="K"/>
</signal>
<signal name="N$43">
<contactref element="RB8" pad="1"/>
<contactref element="RF8" pad="1"/>
<contactref element="CT2" pad="P$2"/>
<contactref element="RB17" pad="1"/>
<contactref element="D12" pad="K"/>
</signal>
<signal name="N$44">
<contactref element="RB9" pad="1"/>
<contactref element="RF9" pad="1"/>
<contactref element="CT1" pad="P$2"/>
<contactref element="RB18" pad="1"/>
<contactref element="D13" pad="K"/>
</signal>
<signal name="LED1_GREEN">
<contactref element="R3" pad="2"/>
<contactref element="STM32F303VE" pad="55"/>
</signal>
<signal name="PC14">
<contactref element="STM32F303VE" pad="8"/>
<contactref element="LSE" pad="P$1"/>
<contactref element="C31" pad="1"/>
</signal>
<signal name="PC15">
<contactref element="STM32F303VE" pad="9"/>
<contactref element="LSE" pad="P$4"/>
<contactref element="C32" pad="1"/>
</signal>
<signal name="CT6">
<contactref element="CF6" pad="2"/>
<contactref element="RF6" pad="2"/>
<contactref element="STM32F303VE" pad="39"/>
</signal>
<signal name="CT5">
<contactref element="CF5" pad="2"/>
<contactref element="RF5" pad="2"/>
<contactref element="STM32F303VE" pad="40"/>
</signal>
<signal name="CT4">
<contactref element="CF4" pad="2"/>
<contactref element="RF4" pad="2"/>
<contactref element="STM32F303VE" pad="41"/>
</signal>
<signal name="CT7">
<contactref element="CF7" pad="2"/>
<contactref element="RF7" pad="2"/>
<contactref element="STM32F303VE" pad="38"/>
</signal>
<signal name="CT8">
<contactref element="CF8" pad="2"/>
<contactref element="RF8" pad="2"/>
<contactref element="STM32F303VE" pad="36"/>
</signal>
<signal name="CT9">
<contactref element="CF9" pad="2"/>
<contactref element="RF9" pad="2"/>
<contactref element="STM32F303VE" pad="35"/>
</signal>
<signal name="D-">
<contactref element="STM32F303VE" pad="70"/>
<contactref element="USB-C" pad="A7"/>
<contactref element="TP6" pad="TP"/>
</signal>
<signal name="D+">
<contactref element="STM32F303VE" pad="71"/>
<contactref element="USB-C" pad="A6"/>
<contactref element="TP5" pad="TP"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="LED2_YELLOW">
<contactref element="R4" pad="2"/>
<contactref element="STM32F303VE" pad="56"/>
</signal>
<signal name="LED3_RED">
<contactref element="R5" pad="2"/>
<contactref element="STM32F303VE" pad="57"/>
</signal>
<signal name="MOSI">
<contactref element="RFM69HCW" pad="12"/>
<contactref element="SJ9" pad="2"/>
<contactref element="SJ17" pad="2"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="RFM69HCW" pad="1"/>
<contactref element="SJ4" pad="2"/>
<contactref element="SJ16" pad="2"/>
<contactref element="SJ6" pad="1"/>
</signal>
<signal name="SPI_CLK">
<contactref element="RFM69HCW" pad="13"/>
<contactref element="SJ10" pad="2"/>
<contactref element="SJ7" pad="1"/>
<contactref element="SJ15" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="PCB2" pad="P$41"/>
</signal>
<signal name="N$24">
<contactref element="PCB2" pad="P$57"/>
</signal>
<signal name="CS_RFM69">
<contactref element="RFM69HCW" pad="14"/>
<contactref element="PCB2" pad="P$64"/>
<contactref element="SJ13" pad="2"/>
</signal>
<signal name="SPI3_CS">
<contactref element="STM32F303VE" pad="77"/>
<contactref element="SJ14" pad="2"/>
</signal>
<signal name="SPI3_MISO">
<contactref element="STM32F303VE" pad="79"/>
<contactref element="SJ16" pad="1"/>
</signal>
<signal name="SPI3_MOSI">
<contactref element="STM32F303VE" pad="80"/>
<contactref element="SJ17" pad="1"/>
</signal>
<signal name="CS_STM32_RPI">
<contactref element="PCB2" pad="P$72"/>
<contactref element="SJ8" pad="1"/>
</signal>
<signal name="USART3_RX">
<contactref element="STM32F303VE" pad="48"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="USART3_TX">
<contactref element="STM32F303VE" pad="47"/>
<contactref element="SJ18" pad="2"/>
</signal>
<signal name="PUSHIN_3">
<contactref element="STM32F303VE" pad="65"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="C20" pad="1"/>
<contactref element="D21" pad="K"/>
</signal>
<signal name="PUSHIN_1">
<contactref element="STM32F303VE" pad="63"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="C1" pad="1"/>
<contactref element="D17" pad="K"/>
</signal>
<signal name="N$31">
<contactref element="R9" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="R18" pad="1"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="R16" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="R11" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="24V">
<contactref element="R9" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="U$2" pad="OUT+"/>
<contactref element="U$6" pad="P$1"/>
</signal>
<signal name="MBUS_RX">
<contactref element="R18" pad="2"/>
<contactref element="SJ11" pad="2"/>
<contactref element="SJ33" pad="2"/>
</signal>
<signal name="MBUS_TX">
<contactref element="R19" pad="2"/>
<contactref element="SJ12" pad="2"/>
<contactref element="SJ31" pad="2"/>
</signal>
<signal name="ADC_RJ45IN">
<contactref element="RJ45_1" pad="8"/>
<contactref element="STM32F303VE" pad="54"/>
</signal>
<signal name="CT6_EX">
<contactref element="STM32F303VE" pad="15"/>
<contactref element="EXPANSION" pad="10"/>
</signal>
<signal name="CT7_EX">
<contactref element="STM32F303VE" pad="16"/>
<contactref element="EXPANSION" pad="9"/>
</signal>
<signal name="VSIG4">
<contactref element="STM32F303VE" pad="17"/>
<contactref element="EXPANSION" pad="11"/>
</signal>
<signal name="VSIG5">
<contactref element="STM32F303VE" pad="18"/>
<contactref element="EXPANSION" pad="12"/>
</signal>
<signal name="SPI3_CS_ESP">
<contactref element="STM32F303VE" pad="84"/>
</signal>
<signal name="IO1_EX">
<contactref element="EXPANSION" pad="15"/>
<contactref element="STM32F303VE" pad="97"/>
</signal>
<signal name="IO3_EX">
<contactref element="EXPANSION" pad="17"/>
<contactref element="STM32F303VE" pad="1"/>
</signal>
<signal name="IO5_EX">
<contactref element="EXPANSION" pad="19"/>
<contactref element="STM32F303VE" pad="3"/>
</signal>
<signal name="IO7_EX">
<contactref element="STM32F303VE" pad="5"/>
<contactref element="EXPANSION" pad="23"/>
</signal>
<signal name="VSIG6">
<contactref element="STM32F303VE" pad="19"/>
<contactref element="EXPANSION" pad="13"/>
</signal>
<signal name="CT1_EX">
<contactref element="STM32F303VE" pad="29"/>
<contactref element="EXPANSION" pad="3"/>
</signal>
<signal name="CT2_EX">
<contactref element="STM32F303VE" pad="30"/>
<contactref element="EXPANSION" pad="6"/>
</signal>
<signal name="CT3_EX">
<contactref element="STM32F303VE" pad="31"/>
<contactref element="EXPANSION" pad="5"/>
</signal>
<signal name="CT4_EX">
<contactref element="STM32F303VE" pad="32"/>
<contactref element="EXPANSION" pad="8"/>
</signal>
<signal name="CT5_EX">
<contactref element="STM32F303VE" pad="33"/>
<contactref element="EXPANSION" pad="7"/>
</signal>
<signal name="N$26">
<contactref element="S11" pad="1"/>
<contactref element="RB18" pad="2"/>
<contactref element="RB9" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="RB8" pad="2"/>
<contactref element="RB17" pad="2"/>
<contactref element="S22" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="RB7" pad="2"/>
<contactref element="RB16" pad="2"/>
<contactref element="S33" pad="1"/>
</signal>
<signal name="PULSE1_RJ45">
<contactref element="RJ45_1" pad="6"/>
<contactref element="C41" pad="1"/>
<contactref element="STM32F303VE" pad="67"/>
</signal>
<signal name="PUSHIN_2">
<contactref element="STM32F303VE" pad="64"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="C19" pad="1"/>
<contactref element="D18" pad="K"/>
</signal>
<signal name="UART1_TX">
<contactref element="SJ21" pad="1"/>
<contactref element="PCB2" pad="P$50"/>
<contactref element="SJ12" pad="1"/>
<contactref element="STM32F303VE" pad="68"/>
<contactref element="UART1" pad="2"/>
</signal>
<signal name="UART1_RX">
<contactref element="SJ20" pad="1"/>
<contactref element="PCB2" pad="P$48"/>
<contactref element="SJ11" pad="1"/>
<contactref element="STM32F303VE" pad="69"/>
<contactref element="UART1" pad="1"/>
</signal>
<signal name="IO2_EX">
<contactref element="EXPANSION" pad="16"/>
<contactref element="STM32F303VE" pad="98"/>
</signal>
<signal name="IO4_EX">
<contactref element="EXPANSION" pad="18"/>
<contactref element="STM32F303VE" pad="2"/>
</signal>
<signal name="IO6_EX">
<contactref element="STM32F303VE" pad="4"/>
<contactref element="EXPANSION" pad="21"/>
</signal>
<signal name="IO8_EX">
<contactref element="STM32F303VE" pad="91"/>
</signal>
<signal name="BUTTON1">
<contactref element="STM32F303VE" pad="53"/>
<contactref element="S1" pad="2"/>
<contactref element="PCB2" pad="P$53"/>
</signal>
<signal name="IO11_EX">
<contactref element="STM32F303VE" pad="95"/>
</signal>
<signal name="N$13">
<contactref element="PCB2" pad="P$66"/>
</signal>
<signal name="RPI_GPIO16">
<contactref element="STM32F303VE" pad="59"/>
<contactref element="SJ29" pad="2"/>
</signal>
<signal name="RPI_GPIO20">
<contactref element="STM32F303VE" pad="60"/>
<contactref element="SJ30" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="STM32F303VE" pad="93"/>
<contactref element="EXPANSION" pad="20"/>
<contactref element="U1" pad="33"/>
<contactref element="SJ26" pad="1"/>
<contactref element="OLED" pad="1"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="STM32F303VE" pad="92"/>
<contactref element="EXPANSION" pad="22"/>
<contactref element="U1" pad="36"/>
<contactref element="SJ27" pad="2"/>
<contactref element="OLED" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R10" pad="1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="TXD0_ESP">
<contactref element="U1" pad="35"/>
<contactref element="SJ3" pad="1"/>
<contactref element="SJ20" pad="2"/>
<contactref element="SV2" pad="5"/>
</signal>
<signal name="RXD0_ESP">
<contactref element="U1" pad="34"/>
<contactref element="SJ18" pad="1"/>
<contactref element="SJ21" pad="2"/>
<contactref element="SV2" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="C16" pad="1"/>
<contactref element="SV2" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="C16" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="25"/>
<contactref element="BOOT_ESP" pad="2"/>
</signal>
<signal name="DIO0">
<contactref element="RFM69HCW" pad="2"/>
<contactref element="PCB2" pad="P$58"/>
<contactref element="STM32F303VE" pad="89"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="HSPI_CLK">
<contactref element="U1" pad="13"/>
<contactref element="SJ10" pad="1"/>
</signal>
<signal name="HSPIQ">
<contactref element="U1" pad="14"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="HSPID">
<contactref element="U1" pad="16"/>
<contactref element="SJ9" pad="1"/>
</signal>
<signal name="HSPICS0">
<contactref element="U1" pad="23"/>
<contactref element="SJ13" pad="1"/>
</signal>
<signal name="SPI3_CLK">
<contactref element="STM32F303VE" pad="78"/>
<contactref element="SJ15" pad="1"/>
</signal>
<signal name="RPI_MOSI">
<contactref element="PCB2" pad="P$59"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="RPI_MISO">
<contactref element="PCB2" pad="P$61"/>
<contactref element="SJ6" pad="2"/>
</signal>
<signal name="RPI_SPI_CLK">
<contactref element="PCB2" pad="P$63"/>
<contactref element="SJ7" pad="2"/>
</signal>
<signal name="CSESP_STM32">
<contactref element="U1" pad="27"/>
<contactref element="SJ19" pad="1"/>
</signal>
<signal name="CS_STM32">
<contactref element="SJ19" pad="2"/>
<contactref element="SJ8" pad="2"/>
<contactref element="SJ14" pad="1"/>
</signal>
<signal name="ANT">
<contactref element="RFM69HCW" pad="8"/>
<contactref element="J$1" pad="SIG"/>
</signal>
<signal name="MBUS_I/O">
<contactref element="R17" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="U$6" pad="P$2"/>
</signal>
<signal name="UART2_RX">
<contactref element="STM32F303VE" pad="26"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="NRST_STM">
<contactref element="STM32F303VE" pad="14"/>
<contactref element="S2" pad="2"/>
<contactref element="SJ25" pad="2"/>
<contactref element="SJ32" pad="1"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="RST_RFM">
<contactref element="RFM69HCW" pad="6"/>
<contactref element="SJ24" pad="2"/>
<contactref element="SJ28" pad="1"/>
</signal>
<signal name="PUSHIN_BYANT">
<contactref element="STM32F303VE" pad="96"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="C22" pad="1"/>
<contactref element="D26" pad="K"/>
</signal>
<signal name="PULSE_2_RJ45">
<contactref element="C46" pad="1"/>
<contactref element="RJ45_2" pad="6"/>
</signal>
<signal name="DS18B20_2_RJ45">
<contactref element="RJ45_2" pad="4"/>
<contactref element="R7" pad="1"/>
<contactref element="STM32F303VE" pad="81"/>
</signal>
<signal name="ADC_2_RJ45IN">
<contactref element="RJ45_2" pad="8"/>
</signal>
<signal name="SDA_RPI">
<contactref element="PCB2" pad="P$67"/>
<contactref element="SJ26" pad="2"/>
</signal>
<signal name="SCL_RPI">
<contactref element="PCB2" pad="P$68"/>
<contactref element="SJ27" pad="1"/>
</signal>
<signal name="RST_RFM_ESP">
<contactref element="U1" pad="28"/>
<contactref element="SJ24" pad="1"/>
</signal>
<signal name="NRST_STM_ESP">
<contactref element="U1" pad="30"/>
<contactref element="SJ25" pad="1"/>
</signal>
<signal name="+3V3_ESP">
<contactref element="U1" pad="2"/>
<contactref element="SJ23" pad="1"/>
</signal>
<signal name="RST_RFM_RPI">
<contactref element="PCB2" pad="P$69"/>
<contactref element="SJ28" pad="2"/>
</signal>
<signal name="NRST_STM_RPI">
<contactref element="PCB2" pad="P$51"/>
<contactref element="SJ32" pad="2"/>
</signal>
<signal name="RPI_GPIO20_RPI">
<contactref element="PCB2" pad="P$78"/>
<contactref element="SJ30" pad="1"/>
</signal>
<signal name="RPI_GPIO16_RPI">
<contactref element="PCB2" pad="P$76"/>
<contactref element="SJ29" pad="1"/>
</signal>
<signal name="VREF+">
<contactref element="STM32F303VE" pad="21"/>
<contactref element="VREF_3V3" pad="1"/>
<contactref element="SJ2" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="R22" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="BOOT0_RPI">
<contactref element="PCB2" pad="P$47"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="Q4" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="MBUS_RX_RPI">
<contactref element="PCB2" pad="P$56"/>
<contactref element="SJ33" pad="1"/>
</signal>
<signal name="MBUS_TX_RPI">
<contactref element="PCB2" pad="P$52"/>
<contactref element="SJ31" pad="1"/>
</signal>
<signal name="HSE_OUT_">
<contactref element="HSE" pad="3"/>
<contactref element="R21" pad="2"/>
<contactref element="C29" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
